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Bartonsham Meadows Site Risk Assessment
Site Grid Ref:
SO 5171 3904




What3Words :
///trap.noting.stand




Site Postcode: 
HR1 2QW


Emergency services access point: 
SO 5209 3929  ///trap.noting.stand


Nearest defibrillator:
Corner TA Centre, opposite Volunteer Inn Pub (also Bleed Control

Kit), Harold Street, Hereford, HR1 2QU

 ///bolts.snacks.arts Not publicly accessible

Call 01432 273 932
Nearest A&E: 

Hereford County Hospital. HR1 2BN. 
///member.loops.charm
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All H&S Requirements are outlined in the Herefordshire Wildlife Trust H&S Policy

	WHO’S AT RISK

Volunteers, staff and contractors/operatives carrying out HWT directed work, public.


	Hazard
	Mitigation

	Steep River Banks

	If carrying out work near/in red zone particularly at high flow times. Follow appropriate safeguards for working  near water. See generic SOP for this hazard.

	Overhead power lines

	· Be aware of these and if working rear overhead lines 
· follow safety procedures stated in relevant generic SOP (Working around overhead/underground services).

	Vehicles on public road at site exits/entrances 

	· Make people aware of danger of moving vehicles when entering or leaving site at relevant exits/entrances.

	Biohazards.eg weils, tetanus, leptospirosis.

	· Make people aware of potential harm and follow specific SOP or dynamic RA for activity.

	Falling branches from large trees

	· Tree safety survey/assessment carried out at appropriate intervals by site owners (CC) and action taken as and when necessary by owners (CC)

	Hidden material/hazardous items in long vegetation

	· Advise contractors of possibility of damage to equipment. If possible carry out preliminary search 

	Personal attack

	· Carry out assessment based on individuals and current circumstances

· Leave no-one isolated on site.

· Mobile phones for lone working or on remote sites.

· Agree safe procedure if working alone – follow Lone Working SOP

	Underground Services: Electricity, Water, Gas

	· Check service maps obtained from utilities companies before starting work.

· Ask utility to identify on site and mark line of service.
· Follow safety procedures in relevant SOP (Working around overhead/underground services).



	Temporary Holes as part of cable burying
	· These should be well marked and obvious but beware of hazard in long vegetaion.


[image: image1.png]